SOIL PROFILE	Project :	Proposed Paint Plant Project at UPSIC Industrial Area, District Bulandshahr, Sikandrabad, Uttar Pradesh
B.H. Location :	Water Table :	4.2m	Term. Depth :	20m	B.H. No.:	1
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

8

7

10

13

17

20

37

0.0

0.9

1.5

2.4

3.0

3.9

4.5

5.4

6.0

6.5

6.9

7.5

8.4

9.0

9.7

9.9

Yellowish brown clayey sandy silt with gravel

Yellowish brown sandy clayey silt with gravel

Yellowish brown clayey silty sand with gravel

Yellowish brown clayey sandy silt

Change of the strata

Brownish Grey silty sand

Brownish Grey silty sand

Change of the strata

Grey sand with silt

32

3

3

0

0

0

0

21

12

52

23

76

71

80

41

65

41

75

24

29

20

6

20

4

2

0

0

0

26

29

25

27

Non

Non

Non

17

20

16

18

Plastic

Plastic

Plastic

1.93

1.97

2.02

2.07

2.03

Sample

10.7

16.4

23.1

22.8

24.5

slip

CD

CD

0.10

0.07

24

26
SOIL PROFILE	Project :	Proposed Paint Plant Project at UPSIC Industrial Area, District Bulandshahr, Sikandrabad, Uttar Pradesh
B.H. Location :	Water Table :	4.2m	Term. Depth :	20m	B.H. No.:	1
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

35

41

40

47

31

26	10.5

11.4

12.0

12.9

13.5

14.4

15.0

15.9

16.5

17.4

18.0

19.7

20.0

Grey sand with silt

Grey sand with silt

Grey sand with silt

Grey sand with traces of silt

Change of the strata

Yellowish brown clayey sandy silt

Change of the strata

Grey sand with traces of silt and gravel

N : Observed SPT values

0

0

0

0

0

2

88

88

86

96

15

89

12

12

14

4

72

9

0

0

0

0

13

0

Non

Non

Non

Non

30

Non

Plastic

Plastic

Plastic

Plastic

20

Plastic	Sample

Sample

Sample

Sample

2.09

2.04	slip

slip

slip

slip

25.9

20.1

CD

0.12

27
SOIL PROFILE	Project :	Proposed Paint Plant Project at UPSIC Industrial Area, District Bulandshahr, Sikandrabad, Uttar Pradesh
B.H. Location :	Water Table :	4m	Term. Depth :	20m	B.H. No.:	2
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

11

7

14

16

32

25

0.0

0.9

1.5

2.4

3.0

3.9

4.5

5.4

5.7

6.0

6.9

7.5

8.4

9.0

9.9

Yellowish brown sandy clayey silt with gravel

Yellowish brown sandy clayey sandy silt

Yellowish brown clayey sandy silt

Change of the strata

Grey sand with traces of silt

Grey sand with traces of silt and gravel

Grey sand with traces of silt

2

0

0

0

2

0

15

23

23

91

89

93

57

63

75

9

9

7

26

14

2

0

0

0

38

31

28

Non

Non

Non

23

21

20

Plastic

Plastic

Plastic

1.93

1.98

2.05

2.03

Sample

Sample

Sample

13.6

17.1

22.9

24.1

slip

slip

slip

CD

0.12

23
SOIL PROFILE	Project :	Proposed Paint Plant Project at UPSIC Industrial Area, District Bulandshahr, Sikandrabad, Uttar Pradesh
B.H. Location :	Water Table :	4m	Term. Depth :	20m	B.H. No.:	2
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test
22

23

27

37

40

47	10.5

11.4

12.0

12.9

13.5

14.4

15.0

15.9

16.5

17.4

18.0

20.0	Grey sand with traces of silt

Grey sand with traces of silt and gravel

Grey sand with traces of silt

Grey sand with traces of silt and gravel

Grey sand with traces of silt

Grey sand with traces of silt

N : Observed SPT values	0

2

0

4

0

0	98

91

97

94

98

98	2

7

3

2

2

2	0

0

0

0

0

0	Non

Non

Non

Non

Non

Non	Plastic

Plastic

Plastic

Plastic

Plastic

Plastic

Sample

Sample

Sample

Sample

Sample

Sample

slip

slip

slip

slip

slip

slip

SOIL PROFILE	Project :	Proposed Paint Plant Project at UPSIC Industrial Area, District Bulandshahr, Sikandrabad, Uttar Pradesh
B.H. Location :	Water Table :	4.2m	Term. Depth :	20m	B.H. No.:	3
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

19

8

20

24

29

29

24

0.0

0.9

1.5

2.4

3.0

3.9

4.5

5.2

5.4

6.0

6.9

7.5

8.4

9.0

9.9

Yellowish brown sandy clayey silt

Yellowish brown clayey sandy silt

Yellowish brown clayey sandy silt

Change of the strata

Grey sand with silt and gravel

Grey sand with traces of silt

Grey sand with traces of silt

Grey sand with traces of silt

0

0

0

2

0

0

0

16

21

49

86

95

91

91

60

69

49

12

5

9

9

24

10

2

0

0

0

0

37

29

25

Non

Non

Non

Non

22

19

15

Plastic

Plastic

Plastic

Plastic

1.98

2.06

1.99

Sample

Sample

Sample

16.2

23.9

20.3

slip

slip

slip

CD

0.08

25
SOIL PROFILE	Project :	Proposed Paint Plant Project at UPSIC Industrial Area, District Bulandshahr, Sikandrabad, Uttar Pradesh
B.H. Location :	Water Table :	4.2m	Term. Depth :	20m	B.H. No.:	3
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

33

30

41

38

36

42

10.5

11.4

12.0

12.9

13.5

14.4

15.0

15.9

16.5

17.4

18.0

20.0

Grey sand with traces of silt

Grey sand with traces of silt and gravel

Grey sand with traces of silt

Grey sand with traces of silt and gravel

Grey sand with traces of silt and gravel

Grey sand with traces of silt

N : Observed SPT values

0

2

0

2

2

0

93

95

97

95

96

97

7

3

3

3

2

3

0

0

0

0

0

0

Non

Non

Non

Non

Non

Non

Plastic

Plastic

Plastic

Plastic

Plastic

Plastic	Sample

Sample

Sample

Sample

Sample

Sample	slip

slip

slip

slip

slip

slip
SOIL PROFILE	Project :	Proposed Paint Plant Project at UPSIC Industrial Area, District Bulandshahr, Sikandrabad, Uttar Pradesh
B.H. Location :	Water Table :	4.2m	Term. Depth :	20m	B.H. No.:	4
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

9

14

17

16

18

15

0.0

0.9

1.5

2.4

3.0

3.9

4.5

5.4

6.0

6.9

7.5

8.4

9.0

9.9

Yellowish brown gravelly clayey sandy silt

Yellowish brown clayey sandy silt

Yellowish brown clayey sandy silt with gravel

Change of the strata

Yellowish brown / br. grey clayey sandy silt

Grey sand with silt

Grey sand with silt

42

0

3

0

0

0

24

17

13

48

80

89

30

75

74

50

20

11

4

8

10

2

0

0

Low

28

29

26

Non

Non

Plastic

19

20

17

Plastic

Plastic

Tube

1.99

2.03

2.08

Sample

Sample

Sample

bent

19.1

24.1

20.3

slip

slip

slip

CD

0.11

24
SOIL PROFILE	Project :	Proposed Paint Plant Project at UPSIC Industrial Area, District Bulandshahr, Sikandrabad, Uttar Pradesh
B.H. Location :	Water Table :	4.2m	Term. Depth :	20m	B.H. No.:	4
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test
34

37

38

39

43

41	10.5

11.4

12.0

12.9

13.5

14.4

15.0

15.9

16.5

17.4

18.0

20.0	Grey sand with traces of silt

Grey sand with traces of silt

Grey sand with traces of silt

Grey sand with traces of silt

Grey sand with traces of silt

Grey sand with traces of silt

N : Observed SPT values	0

0

0

0

0

0	98

95

96

97

95

97	2

5

4

3

5

3	0

0

0

0

0

0

Non

Non

Non

Non

Non

Non	Plastic

Plastic

Plastic

Plastic

Plastic

Plastic

Sample

Sample

Sample

Sample

Sample

Sample

slip

slip

slip

slip

slip

slip

SOIL PROFILE	Project :	Proposed Paint Plant Project at UPSIC Industrial Area, District Bulandshahr, Sikandrabad, Uttar Pradesh
B.H. Location :	Water Table :	4.3m	Term. Depth :	20m	B.H. No.:	5
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

15

14

12

17

18

20

28

0.0

0.9

1.5

2.4

3.0

3.9

4.5

5.4

6.0

6.7

6.9

7.5

8.2

8.4

9.0

9.9

Yellowish brown sandy clayey silt with gravel

Yellowish brown clayey sandy silt

Yellowish brown clayey sandy silt

Yellowish brown clayey sandy silt

Change of the strata

Brownish grey silty sand

Change of the strata

Grey sand with silt

Grey sand with traces of silt

2

0

11

0

0

0

0

17

18

11

36

70

83

97

56

65

70

62

30

17

3

25

17

8

2

0

0

0

36

31

28

26

Non

Non

Non

23

20

18

17

Plastic

Plastic

Plastic

1.99

2.05

2.09

1.97`

Sample

Sample

15.7

13.4

23.8

22.2

slip

slip

CD

CD

0.12

0.08

24

25
SOIL PROFILE	Project :	Proposed Paint Plant Project at UPSIC Industrial Area, District Bulandshahr, Sikandrabad, Uttar Pradesh
B.H. Location :	Water Table :	4.3m	Term. Depth :	20m	B.H. No.:	5
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

31

36

42

38

44

48	10.5

11.4

12.0

12.9

13.5

14.4

15.0

15.9

16.5

17.4

18.0

20.0

Grey sand with traces of silt

Grey sand with traces of silt

Grey sand with traces of silt

Grey sand with traces of silt

Grey sand with traces of silt

Grey sand with traces of silt

N : Observed SPT values

0

0

0

0

0

0

98

96

96

98

97

97

2

4

4

2

3

3

0

0

0

0

0

0

Non

Non

Non

Non

Non

Non

Plastic

Plastic

Plastic

Plastic

Plastic

Plastic	Sample

Sample

Sample

Sample

Sample

Sample

slip

slip

slip

slip

slip

slip
SOIL PROFILE	Project :	Proposed Paint Plant Project at UPSIC Industrial Area, District Bulandshahr, Sikandrabad, Uttar Pradesh
B.H. Location :	Water Table :	4.2m	Term. Depth :	20m	B.H. No.:	6
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

9

11

12

18

20

25

0.0

0.9

1.5

2.4

3.0

3.9

4.5

5.4

6.0

6.9

7.5

8.4

9.0

9.9

Yellowish brown sandy clayey silt with gravel

Yellowish brown clayey sandy silt with gravel

Change of the strata

Grey sand with silt

Grey sand with silt

Grey sand with traces of silt and gravel

Grey sand with traces of silt

9

6

0

0

2

0

16

17

85

89

91

97

57

68

15

11

7

3

18

9

0

0

0

0

32

29

Non

Non

Non

Non

22

20

Plastic

Plastic

Plastic

Plastic

1.97

1.96

2.03

1.99

Sample

Sample

Sample

20.8

16.9

26.7

26.5

slip

slip

slip

CD

CD

0.11

0.03

23

25

SOIL PROFILE	Project :	Proposed Paint Plant Project at UPSIC Industrial Area, District Bulandshahr, Sikandrabad, Uttar Pradesh
B.H. Location :	Water Table :	4.2m	Term. Depth :	20m	B.H. No.:	6
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test
31

36

40

30

39

45	10.5

11.4

12.0

12.9

13.5

14.4

15.0

15.9

16.5

17.4

18.0

20.0	Grey sand with traces of silt

Grey sand with traces of silt and gravel

Grey sand with traces of silt

Grey sand with traces of silt and gravel

Grey sand with traces of silt and gravel

Grey sand with traces of silt

N : Observed SPT values	0

2

0

3

2

0

95

96

98

95

96

98	5

2

2

2

2

2	0

0

0

0

0

0	Non

Non

Non

Non

Non

Non	Plastic

Plastic

Plastic

Plastic

Plastic

Plastic

Sample

Sample

Sample

Sample

Sample

Sample

slip

slip

slip

slip

slip

slip