SOIL PROFILE	Project :	Proposed Project at Sector - 18, Gurugam
B.H. Location :	Water Table :	N.E.	Term. Depth :	25m	B.H. No.:	1
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

18

22

24

24

35

39	0.0

2.7

3.0

3.9

4.5

5.4

6.0

6.7

6.9

7.5

8.4

9.0

9.9

10.5

11.4	Filled-up soil with debris

Change of the strata

Yellowish brown clayey sandy silt with gravel

Yellowish brown clayey sandy silt with gravel

Change of the strata

Yellowish brown clayey silty sand with gravel

Change of the strata

Yellowish brown clayey sandy silt

Yellowish brown clayey sandy silt with gravel

Change of the strata

Yellowish brown clayey silty sand

3

10

7

0

3

0

20

33

51

30

24

53

65

49

33

57

63

39

12

8

9

13

10

8

29

23

Low

27

29

Low

20

16

Plastic

18

20

Plastic

1.98

1.95

1.91

2.05

2.16

1.92

17.8

18.5

16.5

14.8

17.8

11.7

CD

CD

0.10

0.11

28

29
SOIL PROFILE	Project :	Proposed Project at Sector - 18, Gurugram
B.H. Location :	Water Table :	N.E.	Term. Depth :	25m	B.H. No.:	1
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

46

58

54

40

46

67

56	12.0

12.9

13.5

14.4

15.0

15.9

16.5

17.2

17.4

18.0

20.4

21.0

23.4

24.0

25.0

Yellowish brown clayey silty sand

Yellowish brown clayey silty sand

Yellowish brown clayey silty sand with gravel

Change of the strata

Yellowish brown clayey sandy silt with gravel

Yellowish brown clayey sandy silt with gravel

Yellowish brown clayey sandy silt with gravel

Yellowish brown clayey sandy silt with gravel

Observed 'N' Values

0

0

8

2

2

23

2

57

48

49

41

31

20

25

36

48

41

55

60

51

61

7

4

2

2

7

6

12

Low

Low

Low

24

25

24

27

Plastic

Plastic

Plastic

18

18

17

19	2.00

1.92

1.82

1.81

1.87

2.05

1.98	11.6

7.3

7.0

7.4

12.2

14.4

17.4

CD

0.09

30
SOIL PROFILE	Project :	Proposed Project at Sector - 18, Gurugram
B.H. Location :	Water Table :	N.E.	Term. Depth :	25m	B.H. No.:	2
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

18

18

24

28

24

61

0.0

2.7

3.0

3.9

4.5

5.4

6.0

6.9

7.3

7.5

8.4

9.0

9.9

10.5

11.4	Filled-up soil with debris

Change of the strata

Yellowish brown clayey sandy silt with gravel

Yellowish brown clayey sandy silt with gravel

Yellowish brown clayey sandy silt with gravel

Change of the strata

Yellowish brown clayey silty sand

Change of the strata

Yellowish brown clayey sandy silt with gravel

Yellowish brown clayey sandy silt with gravel

4

3

5

0

3

7

26

20

32

50

34

26

56

67

55

40

49

59

14

10

8

10

14

8

30

28

25

24

28

24

20

20

17

17

19

18

1.93

1.95

1.90

2.01

1.90

1.80

10.6

15.9

8.2

14.3

10.3

4.2

CD

CD

0.12

0.11

27

29
SOIL PROFILE	Project :	Proposed Project at Sector - 18, Gurugram
B.H. Location :	Water Table :	N.E.	Term. Depth :	25m	B.H. No.:	2
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

35

46

51

52

55

55

78	11.8

12.0

12.9

13.5

14.4

15.0

15.9

16.5

17.4

18.0

20.4

21.0

23.4

24.0

25.0	Change of the strata

Yellowish brown clayey silty sand

Yellowish brown clayey silty sand

Yellowish brown clayey silty sand with gravel

Change of the strata

Yellowish brown clayey sandy silt with gravel

Yellowish brown clayey sandy silt with gravel

Yellowish brown clayey sandy silt with gravel

Yellowish brown clayey sandy silt with gravel

Observed 'N' Values

0

0

2

3

7

2

10

55

50

51

45

33

46

24

37

42

43

46

54

47

60

8

8

4

6

6

5

6

Low

23

Low

24

25

24

26

Plastic

16

Plastic

17

17

17

18

1.86

1.99

1.98

1.86

1.98

2.00

1.99

7.1

12.6

15.4

7.9

15.4

10.9

9.2

CD

0.10

31
SOIL PROFILE	Project :	Proposed Project at Sector - 18, Gurugram
B.H. Location :	Water Table :	N.E.	Term. Depth :	25m	B.H. No.:	3
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

20

15

28

32

33

29

27

0.0

2.6

3.0

3.9

4.5

5.4

6.0

6.9

7.5

8.4

9.0

9.9

10.5

11.2

11.4	Filled-up soil with debris

Change of the strata

Yellowish brown clayey sandy silt with gravel

Yellowish brown clayey sandy silt with gravel

Change of the strata

Yellowish brown clayey silty sand with gravel

Change of the strata

Yellowish brown clayey sandy silt with gravel

Yellowish brown clayey sandy silt with gravel

Change of the strata

Yellowish brown clayey silty sand with gravel

2

5

2

8

15

3

33

36

54

29

43

56

53

49

34

51

37

33

12

10

10

12

5

8

28

27

26

32

Low

Low

20

19

18

20

Plastic

Plastic

1.94

2.00

2.08

1.91

2.03

21.4

23.1

15.0

19.2

17.5

CD

0.11

27
SOIL PROFILE	Project :	Proposed Project at Sector - 18, Gurugram
B.H. Location :	Water Table :	N.E.	Term. Depth :	25m	B.H. No.:	3
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

28

51

54

48

N>100

48

47	12.0

12.9

13.5

14.4

15.0

15.9

16.5

17.4

18.0

20.4

21.0

22.0

23.4

24.0

25.0

Yellowish brown silty sand

Yellowish brown silty sand with gravel

Yellowish brown silty sand with gravel

Yellowish brown silty sand with gravel

Yellowish brown gravelly silty sand

Change of the strata

Yellowish brown clayey sandy silt with gravel

Yellowish brown clayey sandy silt with gravel

Observed 'N' Values

0

3

17

2

48

3

27

76

75

55

73

27

30

32

24

22

28

25

25

57

35

0

0

0

0

0

10

6

Non

Non

Non

Non

Non

28

Low

Plastic

Plastic

Plastic

Plastic

Plastic

20

Plastic

2.04

1.97

2.08

2.11

1.96

Tube

2.03	16.4

12.6

18.5

17.1

12.3

bent

17.0	CD

CD	0.07

0.08	28

32